The patches in the "proceedWCaution" folder are my latest patches; however, I do not have a Bean and dialed them in with the HD 500, then converted to Bean using jZab's automatic converter.  This seems to have reset the Cab DEP's to 50% across the board making the patches extremely thin, as low cut is now at 260 HZ.  I will get these fixed in a later release.  Thank you.